# :MEASure:EYE:JITTer:UNITs

Eye Jitter Commands

- :MEASure:EYE:JITTer
- :MEASure:EYE:JITTer:DEFine:SIGNal
- :MEASure:EYE:JITTer:DEFine:SIGNal:AUTodetect
- :MEASure:EYE:JITTer:DEFine:UNITs
- :MEASure:EYE:JITTer:FAVorite
- :MEASure:EYE:JITTer:FORMat
- :MEASure:EYE:JITTer:LOCation?
- :MEASure:EYE:JITTer:SOURce
- :MEASure:EYE:JITTer:STATus?
- :MEASure:EYE:JITTer:STATus:DETails?
- :MEASure:EYE:JITTer:STATus:REASon?
- :MEASure:EYE:JITTer:UNITs

## Command Syntax

    :MEASure:EYE:JITTer:UNITs  {SECond | UINTerval}

## Query Syntax

    :MEASure:EYE:JITTer:UNITs?

## Description

Selects the `:MEASure:EYE:JITTer` measurement units: Second (s) or Unit Interval (UI). Set the units before turning the measurement on.