# :DIFF:COPY

:DIFF General Commands

- :DIFF:COLor
- :DIFF:COPY
- :DIFF:CWINdow
- :DIFF:DESKew
- :DIFF:DISPlay
- :DIFF:DMODe
- :DIFF:FCHan?
- :DIFF:PATTern:FILE:GCODe
- :DIFF:PATTern:FILE:NAME
- :DIFF:PATTern:FILE:RELoad
- :DIFF:PATTern:INVert
- :DIFF:PATTern:KPATtern
- :DIFF:PATTern:MODE
- :DIFF:SCHan?
- :DIFF:SIGNal:TYPE
- :DIFF:SNOise:CALibrate
- :DIFF:SNOise:SNValue:LEVel{0:3}?
- :DIFF:STATus?
- :DIFF:TDELay
- :DIFF:UNAMe

## Command Syntax

    :DIFFN:COPY {DIFF<source>}

Where N identifies a specific differential waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 differential waveform 3 (from the pairing of channels 3 and 4) is `DIFF5_3`.

Where <source> identifies a source channel from which to copy settings. <source> is in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 2 channel 2 is `2_2`.

## Description

Copies channels settings from a source channel into the destination channel. Copied settings include the following:

- Scale
- Offset
- Hardware Skew
- Software Delay
- Signal Type Auto Detect and Type
- External Transducer settings
- External Attenuator settings

The copied settings do not include waveform color or any custom waveform name.