# :ACQuire:STOP

:ACQuire Commands

- :ACQuire Subsystem
- :ACQuire:CDISplay
- :ACQuire:COUNt
- :ACQuire:POINts
- :ACQuire:POINts:AUTO
- :ACQuire:RUN
- :ACQuire:SINGle
- :ACQuire:SMODe
- :ACQuire:SRATe
- :ACQuire:SRATe:AUTO
- :ACQuire:STATe?
- :ACQuire:STOP

## Command Syntax

    :ACQuire:STOP

## Description

Stops data acquisition. This command is equivalent to clicking the Stop button. This command does not erase display memory. To clear display memory, use the `:ACQuire:CDISplay` command. Use the `:ACQuire:RUN` command to resume data acquisition. When acquisition is stopped, use the `:ACQuire:SINGle` command to start a single run of capturing waveform data.