# :LTESt:MEASure:SIMage:MONochrome

:LTESt Measurement Screen Image Commands

- :LTESt:MEASure:SIMage:FNAMe
- :LTESt:MEASure:SIMage:FNAMe:AUPDate
- :LTESt:MEASure:SIMage:FNAMe:USTandard
- :LTESt:MEASure:SIMage:FTYPe?
- :LTESt:MEASure:SIMage:IMETadata
- :LTESt:MEASure:SIMage:INVert
- :LTESt:MEASure:SIMage:MONochrome
- :LTESt:MEASure:SIMage:SINClude
- :LTESt:MEASure:SIMage:STATe
- :LTESt:MEASure:SIMage:WINDow

## Command Syntax

    :LTESt:MEASure:SIMage:MONochrome {ON | OFF | 1 | 0}

## Query Syntax

    :LTESt:MEASure:SIMage:MONochrome?

## Query Response

    {1 | 0}

## Description

Turns monochrome screen capture on and off when reporting a screen capture for a measurement limit test. When on, a black and white image will be captured and saved into a file by the `:LTESt:MEASure:SIMage:FNAMe` command. Selecting monochrome automatically inverts the graticule area's background color. Use the `:LTESt:MEASure:SIMage:STATe` command to enable screen captures to be saved when the limit test completes.