# :CHANnel:EYE:XPOSition

:CHANnel EYE Commands

- :CHANnel EYE Commands
- :CHANnel:EYE:BITS
- :CHANnel:EYE:CCOunt
- :CHANnel:EYE:CURSor
- :CHANnel:EYE:CWINdow
- :CHANnel:EYE:DISPlay
- :CHANnel:EYE:PATTern
- :CHANnel:EYE:UIXPosition
- :CHANnel:EYE:UIXRange
- :CHANnel:EYE:UUNits
- :CHANnel:EYE:WINDow:COPY
- :CHANnel:EYE:WINDow:LEFT
- :CHANnel:EYE:WINDow:METHod
- :CHANnel:EYE:WINDow:RIGHt
- :CHANnel:EYE:WINDow:TRACking
- :CHANnel:EYE:WINDow:WIDTh
- :CHANnel:EYE:XPOSition
- :CHANnel:EYE:XSCale

## Command Syntax

    :CHANnelN:EYE:XPOSition <time>

Where N identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 4 channel 2 is `CHANnel4_2`.

<time> is a double.

## Query Syntax

    :CHANnelN:EYE:XPOSition?

## Description

Sets the channel N horizontal time position (center display location) of the real-time eye display.

This command directly affects the real-time eye's horizontal position setting in UI (unit interval) units (see the `:CHANnel:EYE:UIXPosition` command).

To set the horizontal time scale of the real-time eye display in seconds-per-division, use the `:CHANnel:EYE:XSCale` command.