# :WAVeform:CGRade:WCOunt?

:WAVeform CGRade Commands

- :WAVeform:CGRade:ASCii:DATA?
- :WAVeform:CGRade:COLumns?
- :WAVeform:CGRade:INTeger:DATA?
- :WAVeform:CGRade:POINts?
- :WAVeform:CGRade:ROWS?
- :WAVeform:CGRade:STATus?
- :WAVeform:CGRade:STATus:REASon?
- :WAVeform:CGRade:UICount?
- :WAVeform:CGRade:WCOunt?
- :WAVeform:CGRade:XINCrement?
- :WAVeform:CGRade:XML:READ?
- :WAVeform:CGRade:XML:WRITe?
- :WAVeform:CGRade:XORigin?
- :WAVeform:CGRade:YINCrement?
- :WAVeform:CGRade:YORigin?

## Query Syntax

    :WAVeform:CGRade:WCOunt?

## Description

Returns the number of acquired waveforms represented in the real-time eye, color grade/gray scale waveform, or color grade memory identified by the `:WAVeform:SOURce` command.

This is the same waveforms count that can be seen in the graphical user interface's waveform legend.

For real-time eyes, each waveform can have multiple UIs (unit intervals). To get the total UI count represented in a real-time eye or color grade memory of a real-time eye, use the `:WAVeform:CGRade:UICount?` query.