# :MEASure:JITTer:NOISe:UIS?

Noise Bit Count Commands

- :MEASure:JITTer:NOISe:COUNt?
- :MEASure:JITTer:NOISe:COUNt:LEVel
- :MEASure:JITTer:NOISe:COUNt:STATus?
- :MEASure:JITTer:NOISe:COUNt:STATus:DETails?
- :MEASure:JITTer:NOISe:COUNt:STATus:REASon?

## Query Syntax

    :MEASure:JITTerN:NOISe:UIS?

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Description

Returns the number of Unit Intervals on which the noise measurements are based.