# :CGMemory:YOFFset?

:CGMemory Scaling Commands

- :CGMemory:XLEFt?
- :CGMemory:XPOSition?
- :CGMemory:XREFerence?
- :CGMemory:XRIGht?
- :CGMemory:XSCale?
- :CGMemory:XUNits?
- :CGMemory:YBOTtom?
- :CGMemory:YOFFset?
- :CGMemory:YRANge?
- :CGMemory:YSCale?
- :CGMemory:YTOP?
- :CGMemory:YUNits?

## Query Syntax

    :CGMemoryN:YOFFset?

Where N identifies one of eight {1:8} color grade memories. For example, the color grade memory 2 would be identified as `:CGMemory2`.

## Description

Queries the voltage (or Watts) value representing the vertical offset that is stored for the waveform in eye-memory. The offset is located at the center of the display for electrical channels and the second graticule division from the bottom of the display screen for optical channels. It may or may not be the same as Infiniium's current setting. The vertical scale for the waveform can be queried with `:CGMemory:YSCale?` command.