# :MEASure:JITTer:JITTer:DDPWs:STATus:REASon?

Jitter DDPWS Commands

- :MEASure:JITTer:JITTer:DDPWs?
- :MEASure:JITTer:JITTer:DDPWs:STATus?
- :MEASure:JITTer:JITTer:DDPWs:STATus:DETails?
- :MEASure:JITTer:JITTer:DDPWs:STATus:REASon?

## Query Syntax

    :MEASure:JITTerN:JITTer:DDPWs:STATus:REASon?

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Query Response

Refer to the table "Common Reasons for INV or QUES Status".

## Description

Returns a string that explains the reason for a failed `:MEASure:JITTer:JITTer:DDPWs?` measurement. If the measurement was successful, a null string is returned.

Additional information about the failure may be available using the `:MEASure:JITTer:JITTer:DDPWs:STATus:DETails?` sibling query. Use the `:MEASure:JITTer:JITTer:DDPWs:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors