# :MEASure:HORizontal:SLEWrate:UREFerence:VALue

Slew Rate Commands

- :MEASure:HORizontal:SLEWrate
- :MEASure:HORizontal:SLEWrate:EDIRection
- :MEASure:HORizontal:SLEWrate:FAVorite
- :MEASure:HORizontal:SLEWrate:LOCation?
- :MEASure:HORizontal:SLEWrate:OCCurrences
- :MEASure:HORizontal:SLEWrate:REGion
- :MEASure:HORizontal:SLEWrate:SOURce
- :MEASure:HORizontal:SLEWrate:STATus?
- :MEASure:HORizontal:SLEWrate:STATus:DETails?
- :MEASure:HORizontal:SLEWrate:STATus:REASon?
- :MEASure:HORizontal:SLEWrate:UREFerence:STATe
- :MEASure:HORizontal:SLEWrate:UREFerence:VALue

## Command Syntax

    :MEASure:HORizontal:SLEWrate:UREFerence:VALue <time_location>

<time_location> is a double.

## Query Syntax

    :MEASure:HORizontal:SLEWrate:UREFerence:VALue?

## Description

When a user-defined horizontal reference location is enabled (see `:MEASure:HORizontal:SLEWrate:UREFerence:STATe`), this command specifies its time location with respect to the trigger (t = 0) location.