# :CALibrate:CONNection:SKEW:STATus?

:CALibrate Connection Commands

- :CALibrate:CONNection:CLOCk
- :CALibrate:CONNection:ENABled
- :CALibrate:CONNection:EXPort
- :CALibrate:CONNection:IMPort
- :CALibrate:CONNection:SKEW:ENABled
- :CALibrate:CONNection:SKEW:STATus?
- :CALibrate:CONNection:SKEW:STATus:DETails?
- :CALibrate:CONNection:SKEW:STATus:DTEMperature?
- :CALibrate:CONNection:SKEW:STATus:TIME?
- :CALibrate:CONNection:STARt
- :CALibrate:CONNection:STATus?
- :CALibrate:CONNection:STATus:DETails?
- :CALibrate:CONNection:STATus:DTEMperature?
- :CALibrate:CONNection:STATus:TIME?
- :CALibrate:CONNection:TIMebase:ENABled
- :CALibrate:CONNection:TIMebase:EXPort
- :CALibrate:CONNection:TIMebase:IMPort
- :CALibrate:CONNection:TIMebase:STARt
- :CALibrate:CONNection:TRIGger:ENABled
- :CALibrate:CONNection:VERTical
- :CALibrate:CONNection:VERTical:STATus?
- :CALibrate:CONNection:VERTical:STATus:DETails?
- :CALibrate:CONNection:VERTical:STATus:DTEMperature?
- :CALibrate:CONNection:VERTical:STATus:TIME?

## Query Syntax

    :CALibrate:CONNectionN:SKEW:STATus?

Where N identifies a specific instrument by connection number and must be selected from {1:8}.

## Description

Queries the Skew Adjustment status for the indicated connection number.

One of the following response strings is returned:

"CALIBRATED"
  The calibrations are valid.
"UNCALIBRATED"
  At least one calibration is needed.
""
  An empty string is returned if the hardware for the indicated connection number does not exist. An -241,"Hardware missing" error is returned by the `:SYSTem:ERRor:NEXT?` command.

Use the child queries listed in the following table to return details about the current calibration.

Status String Child Queries
Status String | Child Query to Send
--- | ---
Time of last adjustment, Time change since last adjustment, and Temperature change since last adjustment | `:CALibrate:CONNection:SKEW:STATus:DETails?`
Change in temperature | `:CALibrate:CONNection:SKEW:STATus:DTEMperature?`
Change in Time | `:CALibrate:CONNection:SKEW:STATus:TIME?`

## Child Commands

- `:CALibrate:CONNection:SKEW:STATus:DETails?`
- `:CALibrate:CONNection:SKEW:STATus:DTEMperature?`
- `:CALibrate:CONNection:SKEW:STATus:TIME?`