# :MEASure:LLINe:MLOCation:STATus?

Time of Failure Commands

- :MEASure:LLINe:MLOCation?
- :MEASure:LLINe:MLOCation:STATus?
- :MEASure:LLINe:MLOCation:STATus:REASon?

## Query Syntax

    :MEASure:LLINeN:MLOCation:STATus?

Where N identifies one of 64 {1:64} possible limit line tests. For example, `:LLINe23`.

## Query Response

    {CORR | INV | QUES}

CORR
  The measurement result is correct.
INV
  The measurement result is invalid.
QUES
  The measurement result is questionable.

## Description

Queries the status of the `:MEASure:LLINe:MLOCation?` measurement. Use the `:MEASure:LLINe:MLOCation:STATus:REASon?` child query to determine the reason for an invalid or questionable measurement. .

## See Also

- Measurement Errors