# :MEASure:LLINe:LINE:FPOints:STATus?

Specific Failed Points Commands

- :MEASure:LLINe:LINE:FPOints?
- :MEASure:LLINe:LINE:FPOints:STATus?
- :MEASure:LLINe:LINE:FPOints:STATus:REASon?

## Query Syntax

    :MEASure:LLINeN:LINEM:FPOints:STATus?

Where N identifies one of 64 {1:64} possible limit line tests. For example, `:LLINe23`.

Where M identifies one of 16 {1:16} possible limit lines.

## Query Response

    {CORR | INV | QUES}

CORR
  The measurement result is correct.
INV
  The measurement result is invalid.
QUES
  The measurement result is questionable.

## Description

Queries the status of `:MEASure:LLINe:LINE:FPOints?` query which returns the total number of failed data points in a specific limit line. Use the `:MEASure:LLINe:FPOints:STATus:REASon?` child query to determine the reason for an invalid or questionable measurement.

## See Also

- Measurement Errors