# Data Measurements

Measurements

- Time Measurements
- Amplitude Measurements
- Clock Measurements
- Data Measurements
- SNDR Measurements
- PAM Measurements
- FFT Measurements
- User-Defined Measurements
- NRZ Eye Measurements
- PAM Eye Measurements
- Mask Test Commands
- Querying Measurement Results and Statistics

These measurements are optimized for NRZ signals but, as noted, may work with PAM signals.

- :MEASure:DATA:BERatio (Bit Error Ratio)
- :MEASure:DATA:CDRRate (CDR Rate)
- :MEASure:DATA:DRATe (Data Rate)
- :MEASure:DATA:DTIerror (Data TIE)
- :MEASure:DATA:DEEMphasis (Deemphasis)
- :MEASure:DATA:NOISe (Noise)
- :MEASure:DATA:NUINterval (N-UI)
- :MEASure:DATA:PLENgth (Pattern Length)
- :MEASure:DATA:SERatio (Symbol Error Ratio)
- :MEASure:DATA:UINTerval (Unit Interval)
- :MEASure:DATA:UUINterval (UI-UI)