# :CGMemory:UNAMe:UFName

:CGMemory General Commands

- :CGMemory:CLEar
- :CGMemory:COLor
- :CGMemory:CWINdow
- :CGMemory:DISPlay
- :CGMemory:DSTatus?
- :CGMemory:DSTatus:REASon?
- :CGMemory:PERSistence
- :CGMemory:SIGNal:TYPE
- :CGMemory:STATus?
- :CGMemory:UNAMe
- :CGMemory:UNAMe:UFName

## Command Syntax

    :CGMemoryN:UNAMe:UFName

Where N identifies one of eight color grade memories. For example, the color grade memory 2 would be identified as :CGMemory2.

## Description

Automatically sets the gray-scale/color-grade memory's user name to the name of the waveform's source file. If the waveform was loaded from a displayed input channel, the name of the file that was automatically created when the data was loaded is used. To learn about user names, use the default user name, or enter a custom user name, use the `:CGMemory:UNAMe` command.