# :SNOise Subsystem

:SNOise Commands

- :SNOise Subsystem
- :SNOise:CALibrate:CANCel
- :SNOise:CALibrate:CONTinue
- :SNOise:CALibrate:SDONe?

The :SNOise subsystem provides status, continue, and cancel commands for the oscilloscope noise calibrations.

By measuring the oscilloscope noise and slew rate, the oscilloscope is able to calculate the oscilloscope's contributions to jitter and noise and remove it from the reported RJ and RN measurements.