# :WMEMory:LOAD

:WMEMory Loading Commands

- :WMEMory:LOAD
- :WMEMory:LOAD:SOURce
- :WMEMory:FILE:LOAD
- :WMEMory:FILE:NAME

## Command Syntax

    :WMEMoryN:LOAD

Where N identifies one of eight {1:8} possible waveform memories. For example, `:WMEMory4`.

## Description

Loads the selected waveform source into the indicated waveform-memory location. Use the `:WMEMory:LOAD:SOURce` command to select the source. Use the `:WMEMory:DISPlay` command to display the waveform-memory.

To load a waveform file into waveform memory, use the `:WMEMory:LOAD` and `:WMEMory:LOAD:SOURce` commands.

## Example Command Sequence

    :WMEMory2:LOAD:SOURce CHAN1_1
    :WMEMory2:LOAD
    :WMEMory2:DISPlay ON

## Child Commands

- `:WMEMory:LOAD:SOURce` specifies the source waveform on which to perform the measurement.