# :CGMemory:LOAD:SOURce

:CGMemory Loading Commands

- :CGMemory:FILE:LOAD
- :CGMemory:FILE:NAME
- :CGMemory:LOAD
- :CGMemory:LOAD:SOURce

## Command Syntax

    :CGMemoryN:LOAD:SOURce <source_waveform>

Where N identifies one of eight {1:8} color grade memories. For example, the color grade memory 2 would be identified as `:CGMemory2`.

Where <source_waveform> can be one of the following:

- `CHANnel<connection1-8>_<ch1-8>`; With connection 1, the "`1_`" part is optional, and you can simply use `CHANnel<ch1-8>`.
- `DIFF{1:4}`
- `CGMemory{1:8}`
- `FUNCtion{1:64}`

## Query Syntax

    :CGMemory{1:8}:LOAD:SOURce?

## Description

Selects the source waveform to load into color grade memory. Use the `:CGMemory:LOAD` command to actually load the selected source.

## Example Command Sequence

    :CGMemory2:LOAD:SOURce CHAN1_1
    :CGMemory2:LOAD

## Parent Command

- `:CGMemory:LOAD`