# :TRIGger:PWIDth:POLarity

:TRIGger Pulse Width Commands

- :TRIGger:PWIDth:MODE
- :TRIGger:PWIDth:POLarity
- :TRIGger:PWIDth:REND
- :TRIGger:PWIDth:RSTart
- :TRIGger:PWIDth:SOURce
- :TRIGger:PWIDth:WIDTh

## Command Syntax

    :TRIGger:PWIDth:POLarity  {POSitive | NEGative}

## Query Syntax

    :TRIGger:PWIDth:POLarity?

## Description

In the Pulse Width trigger mode (see `:TRIGger:MODE`), this command specifies the polarity of the pulse to trigger on.