# :WMEMory:THReshold:GENeral:UPPer

:WMEMory Threshold Commands

- :WMEMory:TBASe:GENeral:METHod
- :WMEMory:TBASe:RFALl:METHod
- :WMEMory:THReshold:GENeral:AUTO
- :WMEMory:THReshold:GENeral:BASE
- :WMEMory:THReshold:GENeral:COPY
- :WMEMory:THReshold:GENeral:HYSTeresis
- :WMEMory:THReshold:GENeral:LOWer
- :WMEMory:THReshold:GENeral:METHod
- :WMEMory:THReshold:GENeral:MIDDle
- :WMEMory:THReshold:GENeral:PAM:ASLevels
- :WMEMory:THReshold:GENeral:PAM:ASTHresholds
- :WMEMory:THReshold:GENeral:PAM:PAMLevel:LEVel
- :WMEMory:THReshold:GENeral:PAM:THResholds:EYE
- :WMEMory:THReshold:GENeral:PLOWer
- :WMEMory:THReshold:GENeral:PMIDdle
- :WMEMory:THReshold:GENeral:PUPPer
- :WMEMory:THReshold:GENeral:STZero
- :WMEMory:THReshold:GENeral:TOP
- :WMEMory:THReshold:GENeral:TRACking
- :WMEMory:THReshold:GENeral:UPPer
- :WMEMory:THReshold:RFALl:BASE
- :WMEMory:THReshold:RFALl:COPY
- :WMEMory:THReshold:RFALl:LOWer
- :WMEMory:THReshold:RFALl:METHod
- :WMEMory:THReshold:RFALl:PAM:ASLevels
- :WMEMory:THReshold:RFALl:PAM:PAMLevels:LEVel
- :WMEMory:THReshold:RFALl:PLOWer
- :WMEMory:THReshold:RFALl:PUPPer
- :WMEMory:THReshold:RFALl:TOP
- :WMEMory:THReshold:RFALl:TRACking
- :WMEMory:THReshold:RFALl:UPPer

## Command Syntax

    :WMEMoryN:THReshold:GENeral:UPPer amplitude

<amplitude> is a double.

Where N identifies one of eight {1:8} possible waveform memories. For example, `:WMEMory4`.

## Query Syntax

    :WMEMoryN:THReshold:GENeral:UPPer?

## Description

Sets the General threshold's upper threshold-definition level. This value is used when making measurements with custom threshold definitions that are based on absolute amplitude. When custom threshold definitions are based on percent, use the `:WMEMory:THReshold:GENeral:PUPPer` command.

Use the `:WMEMory:THReshold:GENeral:METHod` command to set waveform threshold levels to standard percentages or custom definitions.

Use the `:WMEMory:THReshold:GENeral:MIDDle` command to enter a middle threshold level. Use the `:WMEMory:THReshold:GENeral:LOWer` command to enter a lower threshold level.

## Example Command Sequence

    :WMEMory2:THReshold:GENeral:TRACking OFF
    :WMEMory2:THReshold:GENeral:METHod ABSolute
    :WMEMory2:THReshold:GENeral:UPPer 125E-3
    :WMEMory2:THReshold:GENeral:MIDDle 0E0
    :WMEMory2:THReshold:GENeral:LOWer -125E-3