# :NETWorks:DFILe:DSTatus:REASon?

:NETWorks:DFILe Commands

- :NETWorks:DFILe Commands
- :NETWorks:DFILe:CLEar
- :NETWorks:DFILe:DSTatus?
- :NETWorks:DFILe:DSTatus:REASon?
- :NETWorks:DFILe:ENABle?
- :NETWorks:DFILe:FILE:LOAD
- :NETWorks:DFILe:FILE:NAME
- :NETWorks:DFILe:PTYPe?

## Query Syntax

    :NETWorks:DFILe{1:4}:DSTatus:REASon?

## Query Response

    <string>

## Description

Returns a description of the status of the specified S-parameter memory. If S-parameter data are currently in the specified S-parameter memory location, the name of the source waveform will be returned. For example, "Source: Channel 1_1". If the S-parameter memory is empty, the string "Please select a file." is returned. If the file is corrupt or an incorrect type, the string "Unable to load file." is returned. To check the status of the S-parameter memory, use the `:NETWorks:DFILe:DSTatus?` parent query.