# :CHANnel:PATTern:FILE:NAME

:CHANnel General Commands

- :CHANnel:ATTenuation?
- :CHANnel:COLor
- :CHANnel:COPY
- :CHANnel:COUPling
- :CHANnel:CWINdow
- :CHANnel:DB?
- :CHANnel:DISPlay
- :CHANnel:IMPedance
- :CHANnel:GAIN?
- :CHANnel:PATTern:FILE:GCODe
- :CHANnel:PATTern:FILE:NAME
- :CHANnel:PATTern:FILE:RELoad
- :CHANnel:PATTern:INVert
- :CHANnel:PATTern:KPATtern
- :CHANnel:PATTern:MODE
- :CHANnel:SIGNal:TYPE
- :CHANnel:SKEW
- :CHANnel:SNOise:CALibrate
- :CHANnel:SNOise:SNValue:LEVel{0:3}?
- :CHANnel:SRANge?
- :CHANnel:STATus?
- :CHANnel:UNAMe

## Command Syntax

    :CHANnelN:PATTern:FILE:NAME "filename"

Where N identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 4 channel 2 is `CHANnel4_2`.

## Query Syntax

    :CHANnelN:PATTern:FILE:NAME?

## Query Response

    "string"

## Description

When you have chosen "loading a pattern file" to identify the data signal pattern (see `:CHANnel:PATTern:MODE`), this command lets you specify the name of the file to load. The file name is a quoted full-path string.

If there are changes to the pattern file that has been loaded, use the `:CHANnel:PATTern:FILE:RELoad` command.