# :LTESt:LLINe:SWAVeform:RESet

:LTESt Limit Line Commands

- :LTESt:LLINe:TEST{N}:MODE
- :LTESt:LLINe:TEST{N}:STATe
- :LTESt:LLINe:SIMage:FNAMe
- :LTESt:LLINe:SIMage:FNAMe:AUPDate
- :LTESt:LLINe:SIMage:FNAMe:USTandard
- :LTESt:LLINe:SIMage:FTYPe?
- :LTESt:LLINe:SIMage:IMETadata
- :LTESt:LLINe:SIMage:INVert
- :LTESt:LLINe:SIMage:MONochrome
- :LTESt:LLINe:SIMage:SAVE
- :LTESt:LLINe:SIMage:SINClude
- :LTESt:LLINe:SIMage:STATe
- :LTESt:LLINe:SIMage:WINDow
- :LTESt:LLINe:SSUMmary:FNAMe
- :LTESt:LLINe:SSUMmary:STATe
- :LTESt:LLINe:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:LLINe:SWAVeform:CHANnel:FTYPe
- :LTESt:LLINe:SWAVeform:CHANnel{N}:STATe
- :LTESt:LLINe:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:LLINe:SWAVeform:CMODe{N}:FNAMe
- :LTESt:LLINe:SWAVeform:CMODe:FTYPe
- :LTESt:LLINe:SWAVeform:CMODe{N}:STATe
- :LTESt:LLINe:SWAVeform:CMODe{N}:WMEMory
- :LTESt:LLINe:SWAVeform:DIFF{N}:FNAMe
- :LTESt:LLINe:SWAVeform:DIFF:FTYPe
- :LTESt:LLINe:SWAVeform:DIFF{N}:STATe
- :LTESt:LLINe:SWAVeform:DIFF{N}:WMEMory
- :LTESt:LLINe:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:LLINe:SWAVeform:FUNCtion{N}:STATe
- :LTESt:LLINe:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:LLINe:SWAVeform:RESet

## Command Syntax

    :LTESt:LLINe:SWAVeform:RESet

## Description

Turns off the reporting action to save channel, differential, common-mode, and function waveforms to a file or memory location whenever limit testing for a limit line test stops data acquisition. It is equivalent to sending the following command for each available waveform:

    :LTESt:LLINe:SWAVeform:CHANnel:STATe OFF
    :LTESt:LLINe:SWAVeform:CMODe:STATe OFF
    :LTESt:LLINe:SWAVeform:DIFF:STATe OFF
    :LTESt:LLINe:SWAVeform:FUNCtion:STATe OFF